[admin@MikroTik] > export
# jan/02/1970 00:01:11 by RouterOS 6.15
# software id = UNKW-3HSV
#
/interface bridge
add admin-mac=4C:5E:0C:7A:E5:CF auto-mac=no l2mtu=1598 name=bridge-local
/interface ethernet
set [ find default-name=ether1 ] name=ether1-gateway
set [ find default-name=ether2 ] name=ether2-master-local
set [ find default-name=ether3 ] master-port=ether2-master-local name=\
    ether3-slave-local
set [ find default-name=ether4 ] master-port=ether2-master-local name=\
    ether4-slave-local
set [ find default-name=ether5 ] master-port=ether2-master-local name=\
    ether5-slave-local
    /interface wireless
set [ find default-name=wlan1 ] band=2ghz-b/g/n channel-width=\
    20/40mhz-ht-above disabled=no distance=indoors l2mtu=2290 mode=ap-bridge \
    ssid=r030a
/ip neighbor discovery
    set ether1-gateway discover=no
/interface wireless security-profiles
    set [ find default=yes ] authentication-types=wpa2-psk mode=dynamic-keys \
    wpa2-pre-shared-key=raum030a
/ip hotspot user profile
    set [ find default=yes ] idle-timeout=none keepalive-timeout=2m \
    mac-cookie-timeout=3d
/ip pool
    add name=default-dhcp ranges=192.168.88.10-192.168.88.254
/ip dhcp-server
    add address-pool=default-dhcp disabled=no interface=bridge-local lease-time=\
    10m name=default
/interface bridge port
    add bridge=bridge-local interface=ether2-master-local
    add bridge=bridge-local interface=wlan1
/ip address
    add address=192.168.88.1/24 comment="default configuration" interface=\
    bridge-local network=192.168.88.0
/ip dhcp-client
    add comment="default configuration" dhcp-options=hostname,clientid disabled=\
    no interface=ether1-gateway
/ip dhcp-server network
    add address=192.168.88.0/24 comment="default configuration" dns-server=\
    192.168.88.1 gateway=192.168.88.1
/ip dns
    set allow-remote-requests=yes
/ip dns static
    add address=192.168.88.1 name=router
/ip firewall filter
    add chain=input comment="default configuration" protocol=icmp
    add chain=input comment="default configuration" connection-state=established
    add chain=input comment="default configuration" connection-state=related
    add action=drop chain=input comment="default configuration" in-interface=\
        ether1-gateway
    add chain=forward comment="default configuration" connection-state=\
        established
    add chain=forward comment="default configuration" connection-state=related
    add action=drop chain=forward comment="default configuration" \
        connection-state=invalid
/ip firewall nat
    add action=masquerade chain=srcnat comment="default configuration" \
    out-interface=ether1-gateway to-addresses=0.0.0.0
/ip upnp
    set allow-disable-external-interface=no
/system leds
    set 0 interface=wlan1
/tool mac-server
    set [ find default=yes ] disabled=yes
    add interface=ether2-master-local
    add interface=ether3-slave-local
    add interface=ether4-slave-local
    add interface=ether5-slave-local
    add interface=wlan1
    add interface=bridge-local
/tool mac-server mac-winbox
    set [ find default=yes ] disabled=yes
    add interface=ether2-master-local
    add interface=ether3-slave-local
    add interface=ether4-slave-local
    add interface=ether5-slave-local
    add interface=wlan1
    add interface=bridge-local

							    
