routeros auf neuesten stand bringen

1. router an eth1 oder eth2 anschliessen
2. eth1 mit statischer adresse 192.168.88.2/24 starten
3. auf router anmelden
4. wieder abmelden
5. pc zum nat-router machen:

#Routing einschalten
echo 1 > /proc/sys/net/ipv4/ip_forward
#Nat loeschen
iptables -t nat -F
#Nat neu konfigurieren
iptables -A FORWARD -o eth0 -i eth1 -s 192.168.88.0/24 -m conntrack \
	 --ctstate NEW -j ACCEPT
iptables -A FORWARD -m conntrack --ctstate ESTABLISHED,RELATED -j ACCEPT
iptables -t nat -A POSTROUTING -o eth0 -j MASQUERADE
#Nat Tabelle auflisten
iptables -t nat -n -L

6. dns-server auf router setzen (adresse ggfs. anpassen):
   /ip dns set servers=129.143.2.10

7. default-gw auf router setzen:
   /ip route add  dst-address=0.0.0.0/0 gateway=192.168.88.2 

8. /system package update> check-for-updates
          channel: current
	  current-version: 6.40.5
	  latest-version: 6.40.5
	  status: System is already up to date

9. /system package update download

10. /system reboot

11. wiederanmelden

12. /system package print 

Flags: X - disabled
 #   NAME               VERSION              SCHEDULED
  0   routeros-mipsbe    6.40.5
  1   system             6.40.5
  2   ipv6               6.40.5
  3   wireless           6.40.5
  4   hotspot            6.40.5
  5   dhcp               6.40.5
  6   mpls               6.40.5
  7   routing            6.40.5
  8   ppp                6.40.5
  9   security           6.40.5
  10   advanced-tools     6.40.5
	   
