(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "LS1Pol" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 3.302 -4.318 0))
    (property "Value" "LS1Pol" (id 1) (at 5.588 -2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "LS1Pol_0_1")
    (symbol "LS1Pol_1_1"
      (pin output line (at 0 -10.16 90) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin input line (at 0 5.08 270) (length 5.08)
        (name "L")
        (number "~")
      )
    )
  )
  (symbol "Leiter" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at -3.81 -2.032 0))
    (property "Value" "Leiter" (id 1) (at -4.572 3.048 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "Leiter_0_1")
  )
  (symbol "N" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 2.54 -2.54 0))
    (property "Value" "N" (id 1) (at -5.08 2.54 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "N_0_1")
    (symbol "N_1_1")
  )
  (symbol "N_klein" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at -0.635 -2.54 0))
    (property "Value" "N_klein" (id 1) (at -3.683 2.667 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "N_klein_0_1")
    (symbol "N_klein_1_1")
  )
  (symbol "PE" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 2.54 -2.54 0))
    (property "Value" "PE" (id 1) (at -5.08 2.54 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "PE_0_1")
    (symbol "PE_1_1")
  )
  (symbol "PE_klein" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at -1.27 -2.54 0))
    (property "Value" "PE_klein" (id 1) (at -3.175 2.54 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "PE_klein_0_1")
    (symbol "PE_klein_1_1")
  )
  (symbol "RCBO2Pol" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LSFI" (id 0) (at 6.604 -4.318 0))
    (property "Value" "RCBO2Pol" (id 1) (at 9.398 -2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "RCBO2Pol_0_1")
    (symbol "RCBO2Pol_1_1"
      (pin output line (at -2.54 -10.16 90) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin input line (at -2.54 5.08 270) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin output line (at 2.54 -10.16 90) (length 5.08)
        (name "N")
        (number "~")
      )
      (pin input line (at 2.54 5.08 270) (length 5.08)
        (name "N")
        (number "~")
      )
    )
  )
  (symbol "RCCB2Pol" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "FI" (id 0) (at 6.604 -4.318 0))
    (property "Value" "RCCB2Pol" (id 1) (at 9.398 -2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "RCCB2Pol_0_1")
    (symbol "RCCB2Pol_1_1"
      (pin output line (at -2.54 -10.16 90) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin input line (at -2.54 5.08 270) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin output line (at 2.54 -10.16 90) (length 5.08)
        (name "N")
        (number "~")
      )
      (pin input line (at 2.54 5.08 270) (length 5.08)
        (name "N")
        (number "~")
      )
    )
  )
  (symbol "ausschalter" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 2.286 -4.572 0))
    (property "Value" "ausschalter" (id 1) (at 2.286 -2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "ausschalter_0_1")
    (symbol "ausschalter_1_1"
      (pin output line (at 0 -7.62 90) (length 2.4892)
        (name "~")
        (number "~")
      )
      (pin input line (at 0 2.54 270) (length 2.4892)
        (name "~")
        (number "~")
      )
    )
  )
  (symbol "klemme" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at -3.81 -2.54 0))
    (property "Value" "klemme" (id 1) (at -3.81 2.54 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "klemme_0_1")
  )
  (symbol "klimageraet" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 4.064 -4.572 0))
    (property "Value" "klimageraet" (id 1) (at 4.064 -2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "klimageraet_0_0")
    (symbol "klimageraet_0_1")
    (symbol "klimageraet_1_1"
      (pin input line (at -2.54 5.08 270) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin input line (at 2.54 5.08 270) (length 5.08)
        (name "N")
        (number "~")
      )
      (pin input line (at 0 5.08 270) (length 5.08)
        (name "PE")
        (number "~")
      )
    )
  )
  (symbol "leuchte" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 3.302 -4.826 0))
    (property "Value" "leuchte" (id 1) (at 3.302 -1.27 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "leuchte_0_1")
    (symbol "leuchte_1_1"
      (pin input line (at -2.54 5.08 270) (length 5.08)
        (name "L")
        (number "~")
      )
      (pin input line (at 2.54 5.08 270) (length 5.08)
        (name "N")
        (number "~")
      )
      (pin input line (at 0 5.08 270) (length 5.08)
        (name "PE")
        (number "~")
      )
    )
  )
  (symbol "steckdose1NPE" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 4.826 -2.032 0))
    (property "Value" "steckdose1NPE" (id 1) (at 4.826 2.032 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "steckdose1NPE_0_1")
    (symbol "steckdose1NPE_1_1"
      (pin input line (at 0 5.08 270) (length 3.9878)
        (name "PE")
        (number "1")
      )
      (pin input line (at -2.54 5.08 270) (length 3.9878)
        (name "L")
        (number "2")
      )
      (pin input line (at 2.54 5.08 270) (length 3.9878)
        (name "N")
        (number "3")
      )
    )
  )
  (symbol "steckdose1NPE-3fach" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
    (property "Reference" "LS" (id 0) (at 9.906 -2.54 0))
    (property "Value" "steckdose1NPE-3fach" (id 1) (at 4.572 2.794 0))
    (property "Footprint" "" (id 2) (at -17.78 0 0))
    (property "Datasheet" "" (id 3) (at -17.78 0 0))
    (symbol "steckdose1NPE-3fach_0_1")
    (symbol "steckdose1NPE-3fach_1_1"
      (pin input line (at 0 5.08 270) (length 3.9878)
        (name "PE")
        (number "1")
      )
      (pin input line (at -2.54 5.08 270) (length 3.9878)
        (name "L")
        (number "2")
      )
      (pin input line (at 2.54 5.08 270) (length 3.9878)
        (name "N")
        (number "3")
      )
    )
  )
)
